// eLabComposer version 1.0

//Lab-Drill Information
Language = "English";
labDrill = "True";

//Topics Covered
chapterCovered = "Viewing the Router Interface Information";

//Prompt Information
StepModeArray[0] = "";
StepModeArray[1] = "enable";
StepModeArray[2] = "enable";

//Instruction Information
instructionArray[0] = "The current router possesses a clean, unaltered running-configuration. View the basic configuration and interface details to see the router defaults.";
instructionArray[1] = "View the current running-configuration to look at the default settings.\n\nWhat is the default name given to the router when you first log on?";
instructionArray[2] = "What is the default encapsulation for serial interfaces?\n\nWhat are other encapsulation types supported by your router? \n\nWhat is the default activation status of each interface?\n\nWhat is the command to activate and deactivate an interface?\n\nFind and list three more default settings.";

//Answer Information
assignValueToAnswer(1,"1",False,"show","running-config");
assignValueToAnswer(2,"2",False,"show","interfaces");

//Error Information
assignValueToError(1,"1","Use the command 'show' to display router information.","Use the keyword 'running-config' to specify the current running configuration.");
assignValueToError(2,"2","Use the command 'show' to display router information.","Use the keyword 'interfaces' to specify interface information for all available interfaces.");

//Result Information
assignValueToResult(1,"1","!\n","version 12.0\n","service timestamps debug uptime\n","service timestamps log uptime\n","no service password-encryption\n","!\n","hostname Router\n","!\n","!\n","!\n","!\n","!\n","!\n","memory-size iomem 25\n","ip subnet-zero\n","!\n","!\n","!\n","process-max-time 200\n","!\n","interface Serial0\n"," no ip address\n"," no ip directed-broadcast\n"," shutdown\n","!\n","interface Serial1\n"," no ip address\n"," no ip directed-broadcast\n"," shutdown\n","!\n","interface FastEthernet0\n"," no ip address\n"," no ip directed-broadcast\n"," shutdown\n","!\n","ip classless\n","no ip http server\n","!\n","!\n","line con 0\n"," transport input none\n","line aux 0\n","line vty 0 4\n","!\n","no scheduler allocate\n","end\n","");
assignValueToResult(2,"2","FastEthernet0 is administratively down, line protocol is down\n","  Hardware is PQUICC_FEC, address is 0002.1761.edf8 (bia 0002.1761.edf8)\n","  MTU 1500 bytes, BW 100000 Kbit, DLY 100 usec,\n","     reliability 252/255, txload 1/255, rxload 1/255\n","  Encapsulation ARPA, loopback not set\n","  Keepalive set (10 sec)\n","  Half-duplex, 100Mb/s, 100BaseTX/FX\n","  ARP type: ARPA, ARP Timeout 04:00:00\n","  Last input never, output 00:02:31, output hang never\n","  Last clearing of \"show interface\" counters never\n","  Queueing strategy: fifo\n","  Output queue 0/40, 0 drops; input queue 0/75, 0 drops\n","  5 minute input rate 0 bits/sec, 0 packets/sec\n","  5 minute output rate 0 bits/sec, 0 packets/sec\n","     0 packets input, 0 bytes\n","     Received 0 broadcasts, 0 runts, 0 giants, 0 throttles\n","     0 input errors, 0 CRC, 0 frame, 0 overrun, 0 ignored\n","     0 watchdog, 0 multicast\n","     0 input packets with dribble condition detected\n","     20 packets output, 1653 bytes, 0 underruns\n","     20 output errors, 0 collisions, 0 interface resets\n","     0 babbles, 0 late collision, 0 deferred\n","     20 lost carrier, 0 no carrier\n","     0 output buffer failures, 0 output buffers swapped out\n","Serial0 is administratively down, line protocol is down\n","  Hardware is PowerQUICC Serial\n","  MTU 1500 bytes, BW 128 Kbit, DLY 20000 usec,\n","     reliability 255/255, txload 1/255, rxload 1/255\n","  Encapsulation HDLC, loopback not set\n","  Keepalive set (10 sec)\n","  Last input 00:00:41, output 00:00:36, output hang never\n","  Last clearing of \"show interface\" counters never\n","  Input queue: 0/75/0 (size/max/drops); Total output drops: 0\n","  Queueing strategy: weighted fair\n","  Output queue: 0/1000/64/0 (size/max total/threshold/drops)\n","     Conversations  0/1/32 (active/max active/max total)\n","     Reserved Conversations 0/0 (allocated/max allocated)\n","  5 minute input rate 0 bits/sec, 0 packets/sec\n","  5 minute output rate 0 bits/sec, 0 packets/sec\n","     30 packets input, 2392 bytes, 0 no buffer\n","     Received 30 broadcasts, 0 runts, 0 giants, 0 throttles\n","     1 input errors, 0 CRC, 1 frame, 0 overrun, 0 ignored, 0 abort\n","     68 packets output, 7273 bytes, 0 underruns\n","     0 output errors, 0 collisions, 1 interface resets\n","     0 output buffer failures, 0 output buffers swapped out\n","     0 carrier transitions\n","     DCD=up  DSR=up  DTR=down  RTS=down  CTS=up\n","\n","Serial1 is administratively down, line protocol is down\n","  Hardware is PowerQUICC Serial\n","  MTU 1500 bytes, BW 128 Kbit, DLY 20000 usec,\n","     reliability 255/255, txload 1/255, rxload 1/255\n","  Encapsulation HDLC, loopback not set\n","  Keepalive set (10 sec)\n","  Last input never, output never, output hang never\n","  Last clearing of \"show interface\" counters never\n","  Input queue: 0/75/0 (size/max/drops); Total output drops: 0\n","  Queueing strategy: weighted fair\n","  Output queue: 0/1000/64/0 (size/max total/threshold/drops)\n","     Conversations  0/4/32 (active/max active/max total)\n","     Reserved Conversations 0/0 (allocated/max allocated)\n","  5 minute input rate 0 bits/sec, 0 packets/sec\n","  5 minute output rate 0 bits/sec, 0 packets/sec\n","     0 packets input, 0 bytes, 0 no buffer\n","     Received 0 broadcasts, 0 runts, 0 giants, 0 throttles\n","     0 input errors, 0 CRC, 0 frame, 0 overrun, 0 ignored, 0 abort\n","     3 packets output, 72 bytes, 0 underruns\n","     0 output errors, 0 collisions, 2 interface resets\n","     0 output buffer failures, 0 output buffers swapped out\n","     6 carrier transitions\n","     DCD=down  DSR=down  DTR=up  RTS=up  CTS=down\n","");

//Graphic Information
hasDefaultGraphic = true;
graphicArray[0] = "CCNA2_elab_3_1_4g";
graphicArray[1] = "";
graphicArray[2] = "";

//Router for Step Information
routerUsedForThisStep[0] = 0;
routerUsedForThisStep[1] = 0;
routerUsedForThisStep[2] = 0;

//Router Information
addToRouterSIMObject(0,"Thimphu","","","R1721");
