// eLabComposer version 1.0

//Lab-Drill Information
Language = "English";
labDrill = "True";

//Topics Covered
chapterCovered = "ObservaciÃ³n de la informaciÃ³n de la interfaz del router";

//Prompt Information
StepModeArray[0] = "";
StepModeArray[1] = "enable";
StepModeArray[2] = "enable";

//Instruction Information
instructionArray[0] = "El router actual posee una configuraciÃ³n activa limpia, inalterada. Observe los detalles de la configuraciÃ³n bÃ¡sica y de las interfaces para conocer las configuraciones por defecto del router.";
instructionArray[1] = "Observe la configuraciÃ³n activa actual para conocer las configuraciones por defecto.\n\nÂ¿CuÃ¡l es el nombre por defecto que se le otorga al router al iniciar una sesiÃ³n por primera vez?";
instructionArray[2] = "Â¿CuÃ¡l es el encapsulaciÃ³n por defecto para las interfaces seriales?\n\nÂ¿CuÃ¡les son los otros tipos de encapsulaciÃ³n que admite el router? \n\nÂ¿CuÃ¡l es el estado de activaciÃ³n por defecto de cada interfaz?\n\nÂ¿CuÃ¡l es el comando que se usa para activar y desactivar una interfaz?\n\nBusque y enumere otras tres configuraciones por defecto.";

//Answer Information
assignValueToAnswer(1,"1",False,"show","running-config");
assignValueToAnswer(2,"2",False,"show","interfaces");

//Error Information
assignValueToError(1,"1","Use el comando 'show' para mostrar la informaciÃ³n del router.","Use la palabra clave 'running-config' para especificar la configuraciÃ³n activa actual.");
assignValueToError(2,"2","Use el comando 'show' para mostrar la informaciÃ³n del router.","Use la palabra clave 'interfaces' para especificar la informaciÃ³n de interfaz para todas las interfaces disponibles.");

//Result Information
assignValueToResult(1,"1","!\n","version 12.0\n","service timestamps debug uptime\n","service timestamps log uptime\n","no service password-encryption\n","!\n","hostname Router\n","!\n","!\n","!\n","!\n","!\n","!\n","memory-size iomem 25\n","ip subnet-zero\n","!\n","!\n","!\n","process-max-time 200\n","!\n","interface Serial0\n"," no ip address\n"," no ip directed-broadcast\n"," shutdown\n","!\n","interface Serial1\n"," no ip address\n"," no ip directed-broadcast\n"," shutdown\n","!\n","interface FastEthernet0\n"," no ip address\n"," no ip directed-broadcast\n"," shutdown\n","!\n","ip classless\n","no ip http server\n","!\n","!\n","line con 0\n"," transport input none\n","line aux 0\n","line vty 0 4\n","!\n","no scheduler allocate\n","end\n","");
assignValueToResult(2,"2","FastEthernet0 is administratively down, line protocol is down\n","  Hardware is PQUICC_FEC, address is 0002.1761.edf8 (bia 0002.1761.edf8)\n","  MTU 1500 bytes, BW 100000 Kbit, DLY 100 usec,\n","     reliability 252/255, txload 1/255, rxload 1/255\n","  Encapsulation ARPA, loopback not set\n","  Keepalive set (10 sec)\n","  Half-duplex, 100Mb/s, 100BaseTX/FX\n","  ARP type: ARPA, ARP Timeout 04:00:00\n","  Last input never, output 00:02:31, output hang never\n","  Last clearing of \"show interface\" counters never\n","  Queueing strategy: fifo\n","  Output queue 0/40, 0 drops; input queue 0/75, 0 drops\n","  5 minute input rate 0 bits/sec, 0 packets/sec\n","  5 minute output rate 0 bits/sec, 0 packets/sec\n","     0 packets input, 0 bytes\n","     Received 0 broadcasts, 0 runts, 0 giants, 0 throttles\n","     0 input errors, 0 CRC, 0 frame, 0 overrun, 0 ignored\n","     0 watchdog, 0 multicast\n","     0 input packets with dribble condition detected\n","     20 packets output, 1653 bytes, 0 underruns\n","     20 output errors, 0 collisions, 0 interface resets\n","     0 babbles, 0 late collision, 0 deferred\n","     20 lost carrier, 0 no carrier\n","     0 output buffer failures, 0 output buffers swapped out\n","Serial0 is administratively down, line protocol is down\n","  Hardware is PowerQUICC Serial\n","  MTU 1500 bytes, BW 128 Kbit, DLY 20000 usec,\n","     reliability 255/255, txload 1/255, rxload 1/255\n","  Encapsulation HDLC, loopback not set\n","  Keepalive set (10 sec)\n","  Last input 00:00:41, output 00:00:36, output hang never\n","  Last clearing of \"show interface\" counters never\n","  Input queue: 0/75/0 (size/max/drops); Total output drops: 0\n","  Queueing strategy: weighted fair\n","  Output queue: 0/1000/64/0 (size/max total/threshold/drops)\n","     Conversations  0/1/32 (active/max active/max total)\n","     Reserved Conversations 0/0 (allocated/max allocated)\n","  5 minute input rate 0 bits/sec, 0 packets/sec\n","  5 minute output rate 0 bits/sec, 0 packets/sec\n","     30 packets input, 2392 bytes, 0 no buffer\n","     Received 30 broadcasts, 0 runts, 0 giants, 0 throttles\n","     1 input errors, 0 CRC, 1 frame, 0 overrun, 0 ignored, 0 abort\n","     68 packets output, 7273 bytes, 0 underruns\n","     0 output errors, 0 collisions, 1 interface resets\n","     0 output buffer failures, 0 output buffers swapped out\n","     0 carrier transitions\n","     DCD=up  DSR=up  DTR=down  RTS=down  CTS=up\n","\n","Serial1 is administratively down, line protocol is down\n","  Hardware is PowerQUICC Serial\n","  MTU 1500 bytes, BW 128 Kbit, DLY 20000 usec,\n","     reliability 255/255, txload 1/255, rxload 1/255\n","  Encapsulation HDLC, loopback not set\n","  Keepalive set (10 sec)\n","  Last input never, output never, output hang never\n","  Last clearing of \"show interface\" counters never\n","  Input queue: 0/75/0 (size/max/drops); Total output drops: 0\n","  Queueing strategy: weighted fair\n","  Output queue: 0/1000/64/0 (size/max total/threshold/drops)\n","     Conversations  0/4/32 (active/max active/max total)\n","     Reserved Conversations 0/0 (allocated/max allocated)\n","  5 minute input rate 0 bits/sec, 0 packets/sec\n","  5 minute output rate 0 bits/sec, 0 packets/sec\n","     0 packets input, 0 bytes, 0 no buffer\n","     Received 0 broadcasts, 0 runts, 0 giants, 0 throttles\n","     0 input errors, 0 CRC, 0 frame, 0 overrun, 0 ignored, 0 abort\n","     3 packets output, 72 bytes, 0 underruns\n","     0 output errors, 0 collisions, 2 interface resets\n","     0 output buffer failures, 0 output buffers swapped out\n","     6 carrier transitions\n","     DCD=down  DSR=down  DTR=up  RTS=up  CTS=down\n","");

//Graphic Information
hasDefaultGraphic = true;
graphicArray[0] = "CCNA2_elab_3_1_4g";
graphicArray[1] = "";
graphicArray[2] = "";

//Router for Step Information
routerUsedForThisStep[0] = 0;
routerUsedForThisStep[1] = 0;
routerUsedForThisStep[2] = 0;

//Router Information
addToRouterSIMObject(0,"Thimphu","","","R1721");
